Satellite: EUTELSAT 33E at 33,10°E

BEACON signal: Beacon1: 11702.40 MHz/ X-pol;

Transpondeur: 133

Uplink: Vertical/ Dowlink: Horizontal

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Name | T.S.R | Occ. Bw | Info BitRate | F.E.C | Modulation | Roll Off | Pilot  Insertion | Uplink Freq. Y | Downlink Freq. X | Uplink EIRP at 0 dB/K |
|  | (Msymb/s) | (MHz) | (Mbit/s) |  |  |  |  | (MHz) | (MHz) | (dBW) |
| B | 4,800 | 6 | 10,452 | 3/4 | DVB-S2 8PSK | 0,25 | ON | 14449,160 | 11169,910 | 63,9 |